SECOND HARMONIC GENERATION IN PHOTONIC CRYSTAL FIBER

sh\*Ef dxdy

ESH IS ONE OUTPUT

EF IS ONE OUTPT